A Wavelet Tour of Signal Processing

Stéphane Mallat, Academic Press 1999 (2nd edition)

Figure 11.13: A block of 64 cosine coefficients has the zero frequency (DC) coefficient at the upper left. The run-length makes a zig-zag scan from low to high frequencies.