A Wavelet Tour of Signal Processing

Stéphane Mallat, Academic Press 1999 (2nd edition)

Figure 11.4: Wavelet packet tree that decomposes the frequency interval [0, 22kHz] in 24 frequency bands covered by M = 4 wavelets dilated over six octaves, plus eight low frequency bands of the same bandwidth. The frequency bands are indicated at the leaves in kHz.